FILE: REVISION: DRAWN BY:

PAGE OF

TITLE

5

1 A0 A1 A2 SDA 3 6 n/c 2 7 24Cxx

SCL

U2

net=+3.3V:8 net=GND:4

1 2 X1 12MHz

R17 1M C4

30p

C5

30p

+3.3V

R13 10k usb_io+ usb_io-

R2 1.5k

+3.3V

R121kR111k

+3.3V

R60

+3.3V

R1510k

+3.3V

R4 22

R3 22

R50 do not mount

R7 10k

R8 10k

C3100n

C22.2u

+3.3V

$Revision$ Stefan Petersen (spe@stacken.kth.se) 5 gTAG - uController 2 gTAG-ucont.sch

AVCC 5 18

24 28

25

XCLKSEL

XCLK

CLKOUT

WAKEUP# SCL SDA

16 38

2

DISCON# RESET#

USBD- USBD+

12 4

3

29 30 31 32 33 34 35 36

43 44 45 46 48 49 50 51

42 10

PB0 PB1 PB2 PB3 PB4 PB5 PB6 PB7

PC1 PC2 PC3 PC4 PC5 PC6 PC7

PC0

11

41 37

RDY2 PA4/RDY4 PA5/RDY5

CTL0 CTL2

CY7C64603-52NC

RESERVED1

RESERVED2

RESERVED3

RESERVED4

RESERVED5

RESERVED6

RESERVED7

2223201917159524739262113GND1

GND2

GND3

GND4

GND5

GND6

8AGND

142776XOUT XIN 40VCC1

VCC2

VCC3

VCC4

INCOMPLETE SYMBOL Missing is: * label on pins Errors are: * Wrong pin number size * Distance from pin to pin number (currently 100 pt)

U1

tdo_ttl tdi_ttl tms_ttl tck_ttl trst_ttl

+3.3V

R1610k

R14 10k

+3.3V

R100R90 do not mount

+3.3V

2341510987618201719161514131211CONN1

+3.3V

C6100n

C7100n

C8100n

C9100n

+3.3V

Place one near each VCC pin for U1

This schematic is free software; you can redistribute it and/or modify it under the terms of the GNU General Public License as published by the Free Software Foundation; either version 2 of the License, or (at your option) any later version. This schematic is distributed in the hope that it will be useful, but WITHOUT ANY WARRANTY; without even the implied warranty of MERCHANTABILITY or FITNESS FOR A PARTICULAR PURPOSE. See the GNU General Public License for more details. You should have received a copy of the GNU General Public License along with this program; if not, write to the Free Software Foundation, Inc., 59 Temple Place, Suite 330, Boston, MA 02111 USA

(C) 2001 Stefan Petersen (spe@stacken.kth.se)

21

J1 reset#