{"text_format":"5","workbook":"ods","n_sheets":3,"sheets":["Tabelle1","Tabelle2","Tabelle3"],"props":{"last_modified_by":"gilbert"},"read":"whole","wrapped":"gz","date_system":"iso_in_file"}

{"sheet":"Tabelle1","index":0,"n_rows":73,"n_cols":7,"rows_kept":73}
["# This is the template file for creating symbols with tragesym"]
["# every line starting with '#' is a comment line."]
["# save it as text file with tab separated cells and start tragesym"]
[]
["[options]"]
["# wordswap swaps labels if the pin is on the right side an looks like this:"]
["#   \"PB1 (CLK)\". That's useful for micro controller port labels"]
["# rotate_labels rotates the pintext of top and bottom pins"]
["#   this is useful for large symbols like FPGAs with more than 100 pins"]
["# sort_labels will sort the pins by it's labels"]
["#   useful for address ports, busses, ..."]
["wordswap","yes"]
["rotate_labels","no"]
["sort_labels","yes"]
["generate_pinseq","yes"]
["sym_width",1400]
["pinwidthvertical",400]
["pinwidthhorizontal",400]
[]
["[geda_attr]"]
["# name will be printed in the top of the symbol"]
["# if you have a device with slots, you'll have to use slot= and slotdef="]
["# use comment= if there are special information you want to add"]
["version","20060113 1"]
["name"]
["device"]
["refdes","U?"]
["footprint"]
["description"]
["documentation"]
["author"]
["numslots",0]
["dist-license"]
["use-license"]
["#slot",1]
["#slotdef","1:"]
["#slotdef","2:"]
["#slotdef","3:"]
["#slotdef","4:"]
["#comment"]
["#comment"]
["#comment"]
[]
["[pins]"]
["# tabseparated list of pin descriptions"]
["#"]
["# pinnr is the physical number of the pin"]
["# seq is the pinseq= attribute, leave it blank if it doesn't matter"]
["# type can be (in, out, io, oc, oe, pas, tp, tri, clk, pwr)"]
["# style can be (line,dot,clk,dotclk,spacer,none). none if only want to add a net"]
["# posit. can be (l,r,t,b) or empty for nets."]
["# net specifies the name of the net. Vcc or GND for example."]
["# label represents the pinlabel."]
["#","negation lines can be added with \"\\_\" example: \\_enable\\_ "]
["#","if you want to write a \"\\\" use \"\\\\\" as escape sequence"]
["#"]
["#pinnr","seq","type","style","posit.","net","label"]
["1"]
["2"]
["3"]
["4"]
["5"]
["6"]
["7"]
["8"]
["9"]
["10"]
["11"]
["12"]
["13"]
["14"]
["15"]
["16"]

{"sheet":"Tabelle2","index":1,"n_rows":0,"n_cols":0,"rows_kept":0}

{"sheet":"Tabelle3","index":2,"n_rows":0,"n_cols":0,"rows_kept":0}